# DEPRECATED: example udev rules for the legacy BabyLin USB device.
# Kept for backward compatibility only; new deployments target the MUM adapter
# over Ethernet and do not need a udev rule.
#
# Replace ATTRS{idVendor} and ATTRS{idProduct} with actual values
# Find values with: lsusb

SUBSYSTEM=="usb", ATTRS{idVendor}=="1234", ATTRS{idProduct}=="5678", MODE="0660", GROUP="plugdev", TAG+="uaccess"
